NOR FLAHS need the NOR adapter and nor_V2_xxx.exe ;
NAND FLASH need the NAND adapter and NAND_V2_xx.exe;


"Manual 1>> is the basic use of instructions, please see. 
The programmer does not need to drive, that comes with the windows on the line. 
If the system can not find the device driver, directly ignored. Thank you
Hello When the adapter plate is inserted into the host,
 the white stripes and the outer housing of the adapter are in the same direction as the ProMan signs of the connecting plate and the housing.
First use, please don't put first chip, 
first programmer plug in the USB cable connected to the computer, 
see yellow lamps and lights alternating flashing three. 
If the lights flashing, and flash after the green light,
 that the programmer can start normally. 
 After you can put the chip to read and write.
Put the chip, please try to power off.
 Also please pay attention to the foot of the first chip position (black dots) and on the adapter plate first foot screen printing logo together, please don't put back.
  In addition to the chip pin need to ensure that clean, 
 and in the inside of the elements.
NAND chip, please NAND the transfer board (NAND screen printing) and open the NAND program, nor chip, please use the nor adapter and open the nor.
If you have questions, please use your mobile phone to take pictures of the chip on the inside of the photo, we come to check.
Chip to put the model information, and then check the chip, and then you screenshot (first +PrintScreen key, Ctrl key, +V key Alt), 
we see the results. Thank you
Read the master piece of data,
 please note: unless there is no need for the mother of the data,
  or the mother piece data only read, not erase or write.
The process for reading the master piece of data is: click on the test type information > button, 
then check the redundancy area (default settings) and read bad block data (default settings), 
and then click < read > button. After reading, to read a proofreading >
 <. This is in order to prevent the chip from the poor because of the bad contact and lead to misunderstanding. Generally read two times,
  compared to the same words, to ensure that the reading of the mother piece data is correct.
Because the master slice data is read from a redundant area, 
each 2048 bytes of data area has 64 bytes of redundant area, 
so the file read to the file is more than the actual chip capacity. 
Such as 128M chip, read the file is 132M.